

**Activate CS Unitec's Dust Collection Vacuum from Power Tool On/Off Switch**

The 11 Amp motor of CS Unitec's [Model CS 1225 wet/dry vacuum](http://www.csunitec.com/dust-collection-systems-vacuums/vacuum-dust-collection-systems/cs-1225) provides a strong 130 CFM of airflow with a filtration efficiency of 99.930% to collect debris, dirt and fine dust.

The CS 1225 includes a hose adapter to easily connect portable power tools such as grinders, sanders or saws for dust removal while the tool is in operation. A “Power Take Off” outlet activates the vacuum ON/OFF from the power tool switch and includes a 10-second shut-off delay to clean any dust left in the hose. An automatic shut-off sensor protects the motor and filters during wet vacuuming.

Its Electromagnetic Pulse Filter Cleaning System shakes the filters to remove dust, maximizing suction and doubling filter life. The vacuum senses when the filters are clogged and the suction power or air flow is restricted, cleaning itself when the vacuum is turned on and again when it is turned off. This feature can be set to activate automatically or manually.

A 6.6 gallon tank capacity, 15’ hose and 25’ power cord make the CS 1225 ideal for most construction jobs. Weighing less than 25 pounds, it is portable and convenient to use on the job site or in the shop. A cleaning kit, including wands, nozzles and hose is also available.

*For more information:*

<http://www.csunitec.com/dust-collection-systems-vacuums/vacuum-dust-collection-systems/cs-1225>

***Contact:***

**CS Unitec, Inc.**

Thomas Carroll, President

22 Harbor Avenue

Norwalk, CT 06850

P: 800-700-5919 / 203-853-9522

E: info@csunitec.com

**www.csunitec.com**