

**CS Unitec’s Hydraulic Vertical Grinder**

Grind up to 9” diameter with CS Unitec’s powerful hydraulic vertical grinder. [Model 1 2060 0010](http://www.csunitec.com/saws/underwater-hydraulic-grinders/underwater-hydraulic-vertical-grinder) is ideal for heavy-duty rough grinding and cutting in subsea applications. Features include a protective guard that rotates 360 degrees; wide lever for diver comfort and a second handle to provide stability when working. The 4.75 HP motor has a no-load speed of 3600 RPM and operates on 2000 psi / 12 GPM hydraulic oil.

For more information, please visit: <http://www.csunitec.com/saws/underwater-hydraulic-grinders/underwater-hydraulic-vertical-grinder>

***Contact:***

**CS Unitec, Inc.**

22 Harbor Avenue

Norwalk, CT 06850

P: 800-700-5919 / 203-853-9522

E: info@csunitec.com

**www.csunitec.com**