****

****

**10" Floor Scarifier Tackles Demanding Material Removal Applications**

Tackle the most demanding surface preparation and material removal applications with CS Unitec's Trelawny™ Floor Scarifier. Powered by an 8 HP Honda GX240 gas motor, the [TFP 260 Model 326.2000T](http://www.csunitec.com/surface-preparation/concrete/concrete-metal-scarifiers-hand-held-and-floor-models/floor-scarifiers-and-accessories/10-walk-behind-floor-scarifier) removes coatings and corrosion from concrete and steel surfaces, removes painted lines, roughens concrete and creates a keyed or grooved profile for waterproofing and non-slip surface applications. The TFP 260 is also available with an electric motor – Model 326.2006T.

The TFP 260 has a 10” cutting width and 1/4” maximum cutting depth per pass. Depth control enables removal of surface materials without damaging the substrate, maximizing performance and extending cutter life. Other features include a quick-lift drum lever for operator control and integrated vacuum connection for dust-free scarifying.

CS Unitec offers a selection of cutters for a variety of applications. Tungsten Carbide Tipped cutters are ideal for roughing concrete and heavy corrosion removal, as well as grooving roadways for non-slip surface. Beam cutters remove light paint and corrosion with minimal damage to the substrate. Star cutters are optimal for mastics and rubberized coatings.

<http://www.csunitec.com/surface-preparation/concrete/concrete-metal-scarifiers-hand-held-and-floor-models/floor-scarifiers-and-accessories/10-walk-behind-floor-scarifier>

***Contact:***

**CS Unitec, Inc.**

22 Harbor Avenue

Norwalk, CT 06850

P: 800-700-5919 / 203-853-9522

E: info@csunitec.com

**www.csunitec.com**