

**Drill Holes up to 4” Diameter with CS Unitec’s**

**New Portable Hydraulic Magnetic Drill**

CS Unitec has introduced a new portable hydraulic magnetic drill ideal for use in subsea applications and Ex Zones. With its 3.4 HP reversible motor, [Model 2 1345 0010](http://www.csunitec.com/drills/portable-magnetic-drills-and-drilling-machines/portable-hydraulic-magnetic-drills/model-2-1345-0010-portable-hydraulic-magnetic-drill) produces an infinitely variable speed of 40-250 RPM. This machine has a 12” stroke and can drill holes up to 4” diameter in structural steel and other metals. The drill has a Morse Taper 3 (MT3) chuck, allowing twist drilling up to 1-1/4” dia., tapping up to 1” dia., countersinking up to 2” dia. and reaming up to 1-1/8” dia. Model 2 1345 0010 is ATEX Classified Ex II 2Gc IIB T5 for use in hazardous atmospheres.

The drill’s magnet is manually operated with a lever control. It will continue to maintain a magnetic holding force of up to 1874 lbs. on plate up to 3/8” thickness, even if the drill motor’s power supply is interrupted. At only 50 lbs., this drill is portable to the jobsite.

An optional pipe clamp (Part No. 2 1330 8500) allows for right-angle drilling of steel, cast iron, cement and plastic pipes up to 43-1/4” dia. with additional extension chains.

For more information and complete specifications, please visit: <http://www.csunitec.com/drills/portable-magnetic-drills-and-drilling-machines/portable-hydraulic-magnetic-drills/model-2-1345-0010-portable-hydraulic-magnetic-drill>

***Contact:***

**CS Unitec, Inc.**

22 Harbor Avenue

Norwalk, CT 06850

P: 800-700-5919 / 203-853-9522

E: info@csunitec.com

**www.csunitec.com**