

**CS Unitec's ETS 225 Drywall Sander with Dust Collection Sands Directly to the Edge**

Lightweight and ideal for tight spaces and small rooms, CS Unitec's [ETS 225](http://www.csunitec.com/surface-preparation/drywall-plaster-wood-and-more/drywall-sanders/drywall-sander-9-dia) drywall sander features a special dust hood with detachable segment permitting sanding into corners. Its dust-free sanding discs have vacuum holes and a hook-and-loop backing. Coupled with a dust extraction vacuum, these discs reduce airborne dust for a cleaner and safer working environment. The 9" disc diameter is ideal for sanding large surface areas such as walls, ceilings, wood floors, boats, vehicles and other applications. Light weight (just 6 lbs.) and a special ergonomic handle design allow it to be guided for long periods of time, with less fatigue, both on walls and overhead on ceilings.

The ETS 225 has a 6 Amp, variable-speed motor that operates from 0-2300 RPM and has a lock-on button for continuous use. Standard equipment includes one 80-grit and one 100-grit Corundum sanding disc, one 80-grit nylon screen sanding disc and a carrying case. Additional Corundum sanding discs are available in grits of 40, 60, 80, 100, 120, 150, 180 and 220 for sanding joint compound, paint, lacquer and wood. Nylon Screen sanding discs are available in grits of 80 and 120 and are ideal for sanding joint compound, lacquer, plastics and soft aluminum.

*For more information:*

<http://www.csunitec.com/surface-preparation/drywall-plaster-wood-and-more/drywall-sanders/drywall-sander-9-dia>

***Contact:***

**CS Unitec, Inc.**

Thomas Carroll, President

22 Harbor Avenue

Norwalk, CT 06850

P: 800-700-5919 / 203-853-9522

E: info@csunitec.com

**www.csunitec.com**