# CS Unitec Logo_72





FOR IMMEDIATE RELEASE:

**CS Unitec’s Ultra Compact Magnetic Drill is Ideal for Drilling Holes**

**up to 1-1/2” dia. in Tight Spaces**

Designed with a horizontal motor mount, CS Unitec’s new MAB 155 portable magnetic drill is ideal for drilling in tight spaces. This ultra compact (7” tall) and lightweight (24 lbs.) drilling machine is easily portable to the jobsite, making it the hole-cutting solution for steel fabricators, contractors, plant maintenance and truck body operations. Its powerful 9.25 Amp/110 Volt double-insulated motor has a no-load speed of 460 RPM. It drills up to 1-1/2” dia., 1-1/2” depth with annular cutters in structural steel and other metals. The drill accepts cutters with a 3/4” Weldon shank.

The MAB 155 magnetic drill is equipped with an integrated automatic cooling/lubrication system that increases the life of annular cutters by reducing friction and wear. The unit’s ratchet-style advancing lever can be mounted on the left or right side.

The high-density, dual-coil magnet has a holding strength of up to 2,640 pounds, providing the pulling power required for heavy-duty drilling. The Electronic Safety Shutoff Sensor automatically shuts down the drill motor if the magnet loses contact with the material, protecting the operator and equipment. An internal cable routing system increases safety by helping to protect the motor power cord from external damage.

For more information and to view demo videos, visit CS Unitec's website at:

<https://www.csunitec.com/drills/portable-magnetic-drills-and-drilling-machines/mab-series-electric/mab-155-ultra-compact-portable-magnetic-drill>

Contact: Tom Carroll From: CS Unitec, Inc.

President 22 Harbor Avenue

Norwalk, CT 06850

Email: info@csunitec.com Phone: (800) 700-5919

Website: www.csunitec.com Fax: (203) 853-9921

*For media inquiries contact Jennifer Neale • Les Howe Associates • 860-267-6651 • jneale@leshowe.com*