

****

**CS Unitec Introduces Compact, Portable Magnetic Drill with Automatic Feed and Reverse**

CS Unitec has introduced a new model to their MAB line of portable magnetic drills. The [AutoMAB 450](https://www.csunitec.com/drills/portable-magnetic-drills-and-drilling-machines/mab-series-electric/automab-450) features an automatic feed mechanism with automatic reverse and shutoff.

Ideal for steel fabricators, contractors and plant maintenance professionals, the AutoMAB 450 drills holes up to 1-3/4” diameter with annular cutters in structural steel and other metals. Drilling depth is 2-3/8” maximum with a pilot pin and 4-3/8” without a pilot pin. An integrated automatic cooling/lubrication system increases the life of the annular cutters by reducing friction and wear. Designed for continuous use, the drill operates at 250 or 450 RPM. Its power feed controls drill pressure to maintain optimal RPM and feed rate.

The AutoMAB 450 is equipped with the SAFEMAG™ System which determines whether the magnet has sufficient adhesive force on the material and alerts the user with LED indicators – green for go, red for stop. The Electronic Safety Shutoff Sensor automatically shuts down the drill motor if the magnet loses contact with the material. Additional safety features include simple arrangement of controls for one-handed operation and LED load indicators.

For more information and to view demo videos, visit CS Unitec's website at:

<https://www.csunitec.com/drills/portable-magnetic-drills-and-drilling-machines/mab-series-electric/automab-450>

***Contact:***

**CS Unitec, Inc.**

Thomas Carroll, President

22 Harbor Avenue

Norwalk, CT 06850

P: 800-700-5919 / 203-853-9522

E: info@csunitec.com

**www.csunitec.com**